## Stereo Sound System

#### Speaker Replacement

22-213

Door Speaker:

1. Remove the door panel (see page 20-152).
2. Pull the top of the speaker (A) straight out to release the upper clip, then lift the speaker straight up to release the lower clips.

Front Door:

Rear Door:

3. Disconnect the 2P connector (B) and remove the speaker.

Rear (4-door):

1. Remove the rear shelf (see page 20-65).
2. Remove the three mounting screws, then disconnect the 2P connector (A) from the speaker (B).