## Power Distribution

#### Fuse to Components Index

22-8

Under-dash Fuse/Relay Box

Fuse Number | Amps | Wire Colour | Component(s) or Circuit(s) Protected
1 | 15A | BLK/WHT | Ignition coils
2 | - | - | Not used
3 | 20A | - | Not used
4 | 10A | BLK/ORN | Alternator, ELD unit, EVAP purge control solenoid valve, Primary HO2S, Secondary HO2S, Vehicle speed sensor, Reverse lockout solenoid, CMP sensor
5 | 7.5A | Fuse/relay box socket | Multiplex control unit
6 | 7.5A | YEL/GRN | Headlight adjuster switch, Headlight adjuster unit, Power window master switch
7 | 20A | - | Not used
8 | 7.5A | Fuse/relay box socket | Optional connector V, Multiplex control unit
9 | 10A | GRN | Rear window wiper motor, Rear window washer motor, Rear window intermittent wiper control unit
10 | 7.5A | Fuse/relay box socket | Multiplex control unit
YEL | Back-up lights, EPS control unit, Gauge assembly, Keyless receiver unit, Security control unit
11 | 7.5A | BLK/ORN | ABS modulator-control unit
12 | - | - | Not used
13 | 10A | PNK | SRS unit
14 | 10A | Fuse/relay box socket | Optional connector V
BLK/YEL | Blower motor relay, Heater control panel, Power mirror actuator, Power mirror defogger, Radiator fan relay, Rear window defogger relay, Recirculation control motor
15 | 30A | - | Not used
16 | 20A | - | Not used
17 | 15A | BLK/YEL | Inertia switch, SRS unit
YEL/BLK | ECM, Fuel pump
18 | 15A | YEL/GRN | Cigarette lighter
19 | 7.5A | YEL/BLK | Turn signal/hazard relay
20 | 20A | Fuse/relay box socket | Multiplex control unit
GRN/BLK | Windshield wiper motor, Windshield washer motor
21 | - | - | Not used
22 | 20A | GRN/BLK | Passenger's power window motor
23 | 20A | GRN/WHT | Driver's power window motor
24 | - | - | Not used
25 | - | - | Not used

a a a