## Frame Repair Chart

#### Top View

4-4

Unit: mm (in.) ø: Inner diameter | a b1 b2 b3 c1

c2

c3

d

For sub-frame ø15 (0.59)

For engine mount ø13 (0.51)

For engine mount ø13 (0.51)

For engine mount ø13 (0.51)

For transmission mount ø15 (0.59)

For transmission mount ø15 (0.59)

For transmission mount ø13 (0.51)

For damper mount ø11.5 (0.45)

e

f

g

h

I

j

k

Damper centre ø78 (3.07)

For damper mount ø11.5 (0.45)

For damper mount ø11.5 (0.45)

For sub-frame ø11 (0.43)

For sub-frame ø15 (0.59)

Locate hole ø25 (0.98)

Locate hole ø50 (1.97)

a a a