## Power Distribution

#### Fuse to Component Index (cont'd)

22-10

Under-dash Fuse/Relay Box

Fuse Number | Amps | Wire Colour | Component(s) or Circuit(s) Protected
1 | - | - | Not used
2 | - | - | Not used
3 | - | - | Not used
4 | - | - | Not used
5 | 7.5A | Fuse/relay box socket | Multiplex control unit
6 | 7.5A | YEL/GRN | Headlight adjuster switch, Headlight adjuster unit, Power window master switch, Sunroof open relay, Sunroof close relay, Power window relay
7 | 20A | GRN | Sunroof motor
8 | 7.5A | Fuse/relay box socket | Optional connector V, Multiplex control unit
YEL/RED | Audio unit
9 | 10A | GRN | Rear wiper motor, Rear washer motor
10 | 7.5A | Fuse/relay box socket | Multiplex control unit
YEL | Back-up lights, EPS control unit, Gauge assembly, Keyless receiver unit, Security control unit, Immobiliser control unit
11 | 7.5A | BLK/ORN | ABS modulator-control unit
12 | - | - | Not used
13 | 10A | PNK | SRS unit
14 | 10A | Fuse/relay box socket | Optional connector V
BLK/YEL | Fan control relay, Blower motor relay, Condenser fan relay, Climate control unit (with auto A/C), Heater control panel (without auto A/C), Power mirror actuator, Power mirror defogger, Radiator fan relay, Rear window defogger relay, Recirculation control motor, Seat heater main relay
15 | 30A | RED/YEL | Headlight washer control unit
16 | 20A | RED/BLK | Driver's seat heater, Passenger's seat heater
17 | 15A | BLK/YEL | Inertia switch, SRS unit
18 | 15A | YEL/GRN | Cigarette lighter
19 | 7.5A | YEL/BLK | Turn signal/hazard relay
20 | 30A | Fuse/relay box socket | Multiplex control unit
GRN/BLK | Windshield wiper motor, Windshield washer motor
21 | - | - | Not used
22 | 20A | GRN/BLK | Front passenger's power window motor
23 | 20A | GRN/WHT | Driver's power window motor
24 | 20A | YEL/RED | Left rear power window motor
25 | 20A | YEL/BLU | Right rear power window motor

a a a