## Exterior Trim

#### Side Sill Protection Tape Replacement

20-256

1. Slowly peel up the old side sill protection tape.

2. Clean the body bonding surface with a sponge dampened in alcohol. After cleaning, keep oil, grease and water from getting on the surface.
3. Peel the adhesive backing from the side sill protection tape.
4. Align the alignment marks (A) of the side sill protection tape (B) with the body line (C), then press the tape into place.

5. Remove the application tape.