## Automatic Transmission

#### System description (cont'd)

14-69

Shift Lever Mechanism: 5-door Model

The shift lever has 7 positions: , , , , , and and shifts between positions along the gate in the A/T gear position indicator panel. The shift lever can shift out of position and into position from without pressing or pulling the shift lever. The shift lock/reverse lock mechanism is an additional shift lever lockout mechanism. The shift lever sifts the transmission into , , , , and positions using the shift cable connected between the shift lever and the transmission control shaft. When the shift lever shifts into position, the shift lever is moved to left from position and it pushes the D3 switch to turn ON. Then the transmission shifts into D3 positioNmode, but the shifting position in the transmission is held in position.

1. SHIFT LOCK RELEASE
2. SHIFT LOCK STOP
3. SHIFT LEVER
4. A/T GEAR POSITION INDICATOR PANEL
5. REVERSE LOCK STOP
6. D3 SWITCH
7. SHIFT LEVER BRACKET BASE
8. SHIFT LOCK SOLENOID