## Cylinder Head

#### Cylinder Head Removal (cont'd)

6-17

1. Remove the Following Parts for Removal of the Cylinder Head:

- Remove brackets (A)
- Remove retainer; injector (B)
- Remove injectors (C)
- Remove bracket (D)
- Remove retainer camshaft oil seal (E)
- Remove brackets; camshaft (F)
- Remove camshaft assembly: intake (G)
- Remove camshaft assembly: exhaust (H)
- Remove bolts camshaft carrier fixing (I)
- Remove camshaft carrier (J)
- Remove gasket: camshaft carrier (K)
- Remove bolts: cylinder head fixing (L)
- Remove cylinder head assembly (M)
- Remove gasket: cylinder head (N)

a a a