## ABS Components

#### DTC Troubleshooting (cont'd)

19-107

DTC 31, 32, 33, 34, 35, 36, 37, 38: Solenoid

1. Clear the DTC (see page 19-90).
2. Turn the ignition switch ON (II).
3. Verify the DTC.

Does the ABS indicator come on and are DTCs 31, 32, 33, 34, 35, 36, 37, 38 indicated?

YES - Check for loose terminals in the ABS control unit 25P connector. If necessary, substitute a known-good ABS modulator-control unit and recheck.

NO - The system is OK at this time.

DTC 41, 42, 43, 44: Wheel Lock

1. Check for brake drag.

Do the brakes drag?

YES - Repair the brake drag.

NO - Go to step 2.

2. Check the installation of the appropriate wheel sensor (see table).

   DTC | Appropriate Terminal
   41 | Right-front
   42 | Left-front
   43 | Right-rear
   44 | Left-rear

Is it correct?

YES - The probable cause was the vehicle spun during cornering. If the problem recurs, check the modulator using the Honda PGM Tester.

NO - Reinstall the wheel sensor correctly.