## Honda Multi Matic Transmission/CVT

#### System Description (cont'd)

14-261

, and Position (Forward Range)

- Forward clutch: engaged
- Reverse brake: released
- Start clutch: engaged
- Hydraulic pressure is applied to the forward clutch and the start clutch and the sun gear drives the forward clutch.
- The forward clutch drives the drive pulley shaft, which drives the driven pulley shaft linked by the steel belt.
- The driven pulley shaft drives the secondary drive gear via the start clutch.
- Power is transmitted the secondary driven gear and final drive gear, which in turn drives the final driven gear.

  1. FLYWHEEL
  2. DRIVE PULLEY SHAFT
  3. STEEL BELT
  4. DRIVE PULLEY
  5. FORWARD CLUTCH
  6. REVERSE BRAKE
  7. PLANETARY CARRIER
  8. PINION GEAR
  9. INPUT SHAFT
  10. SUN GEAR
  11. RING GEAR
  12. DRIVEN PULLEY GEAR
  13. DRIVEN PULLEY
  14. SECONDARY DRIVE GEAR
  15. SECONDARY DRIVEN GEAR
  16. FINAL DRIVEN GEAR
  17. FINAL DRIVE GEAR
  18. START CLUTCH