## Engine Assembly

#### Engine Removal (cont'd)

5-8

29. Remove the shift cable covers (A), then remove the shift control cable (B) (A/T).

30. Disconnect the suspension lower arm joints and stabiliser, refer to the '01 Civic Shop Manual on this CD (see page 18-18).
31. Remove the drivehafts, refer to the '01 Civic Shop Manual on this CD (see page 16-3). Coat all precision finished surface with clean engine oil. Tie plastic bags over the driveshaft ends.

32. Lower the hoist.
33. Remove the ground cable (A), upper radiator hose (B), lower radiator hose (C) and heater hose (D).