## Front Wheelhouse/Damper Housing

#### Removal

3-39

- Cut and remove the wheelhouse upper member, and replace the front wheelhouse.

  1. DAMPER HOUSING
  2. WHEELHOUSE UPPER EXTENSION
  3. WHEELHOUSE UPPER MEMBER Reused.
  4. FRONT WHEELHOUSE
  5. ENGINE MOUNT BRACKET
  6. FRONT SIDE FRAME

- Check the wheelhouse upper extension and damper housing for position and damage. If Necessary, remove the wheelhouse upper member and replace the damper housing and wheelhouse upper extension as an assembly. If possible.

  1. DAMPER HOUSING
  2. WHEELHOUSE UPPER EXTENSION
  3. WHEELHOUSE UPPER MEMBER EXTENSION
  4. WHEELHOUSE UPPER MEMBER Reused.