## Exterior Trim

#### Emblem Replacement

20-2

NOTE:

- When removing the emblem, take care not to scratch the body.
- 5-door: For the front and rear ''H''emblems, refer to the '01 Civic Shop Manual, P/N 62S5A00 on this CD (see page 20-257).
- 3-door: For the front and rear ''H''emblems, refer to the '01 Civic Shop Manual Supplement, P/N 62S5A22 on this CD (see page 20-43).

1. Clean the body surface with a sponge dampened in alcohol. After cleaning, keep oil, grease and water from getting on the surface.

1. Apply the emblem, where shown.

   5-door:

1. FRONT "H" EMBLEM
2. CIVIC EMBLEM
3. CTDi EMBLEM
4. REAR "H" EMBLEM

Unit: mm (in.)

[A] : Measure along the tailgate surface.

a a a