## Honda Multi Matic Transmission/CVT

#### Shift Lever Disassembly/Reassembly

14-342

1. SHIFT LEVER KNOB
2. A/T GEAR POSITION INDICATOR PANEL
3. SHIFT LEVER COVER
4. A/T GEAR POSITION INDICATOR PANEL LIGHT BULB
5. SILICONE GREASE
6. SHIFT LEVER BRACKET BASE
7. SILICONE GREASE
8. BUSHING

   SILICONE GREASE

9. A/T GEAR POSITION INDICATOR PANEL BRACKET
10. SCREW

    3 Nm (0.3 kgf/m, 2 lbf/ft)

    Apply non-hardening thread lock sealant.