## Body

####

Seats

Front Seat Cover Replacement | 20-2

Bumpers

Front Bumper Under Spoiler Replacement | 20-6
Rear Bumper Under Spoiler Replacement | 20-7

Exterior Trim

Front Grille Replacement | 20-8
Side Sill Panel Replacement | 20-9
Tailgate Spoiler Replacement | 20-11
Emblem/Sticker Replacement | 20-12

Fenderwell

Rear Strake Replacement | 20-13

Frame

Performance Rod Replacement | 20-14

NOTE: Refer to the 2001 Civic Shop Manual, P/N 62S5A00 and 2001 Civic Shop Manual Supplement, P/N 62S5A20, P/N 62S5A21, P/N 62S5A22 for the items not shown in this manual.

Outline of 3-door Model Changes

- The Civic 3-door Type R model has been added.

- The front seat-back cover replacement procedure is different.
- The front and rear bumper under spoilers have been added.
- The front grille is different.
- The side sill panel has been added.
- The tailgate spoiler is different.
- The Type R emblems and stickers have been added.
- The rear strake is different.
- Some performance rods have been added.

SUPPLEMENTAL RESTRAINT SYSTEM (SRS) (If body maintenance is required)

This model has an SRS which includes a driver's airbag in the steering wheel hub, a passenger's airbag in the dashboard above the glove box, seat belt tensioners in the front seat belt retractors. Information necessary to safely service the SRS is included in the Shop Manual, P/N 62S5A00. Items marked with an asterisk (*) on the contents page include, or are located near, SRS components. Servicing, disassembling or replacing these items will require special precautions and tools, and should therefore be done by an authorised Honda dealer.

WARNING

- To avoid rendering the SRS inoperative, which could lead to personal injury or death in the event of a severe frontal collision, all SRS service work must be performed by an authorised Honda dealer.
- Improper service procedures, including incorrect removal and installation of the SRS, could lead to personal injury caused by unintentional deployment of the airbags.
- Do not bump the SRS unit. Otherwise, the system may fail in a collision, or airbags may deploy when the ignition switch is ON (II).
- SRS electrical wiring connectors are identified by yellow colour coding. Related components are located in the steering column, front console, dashboard, dashboard lower panel, and in the dashboard above the glove box. Do not use electrical test equipment on these circuits.

a a a