## Manual Transmission

#### Mainshaft Reassembly (cont'd)

13-33

1. Install the 5th/6th synchro hub (A) using the special tools.

1. Install the 5th/6th synchro sleeve.

1. Install the synchro spring (A).

1. Install the double cone synchro assembly (B) by aligning the synchro cone fingers (C) with the grooves in 5th/6th synchro hub (D).

1. Install the distance collar and the needle bearing.

1. Install the 6th gear (A) by aligning the synchro cone fingers (B) with the holes in 6th gear (C).

1. Install the new ball bearing (A) using the special tools and a press (B).

a a a