## Exterior Lights

#### Combination Light Switch Test/Replacement (cont'd)

22-113

5. Inspect the connector terminals to be sure they are all making good contact.

- If the terminals are bent, loose or corroded, repair them as necessary and recheck the system.
- If the terminals look OK, check for continuity between the terminals in each switch position according to the tables.

- If there is no continuity, replace the switch.

Light Switch:

Turn Signal Switch:

Front/Rear Fog Lights Switch (KH model):

Rear Fog Light Switch (KG, KE and KB models):