## SRS

#### DTC Troubleshooting Index (cont'd)

23-43

DTC | Detection Item | Notes
5-1 | Internal failure of SRS unit | (see page 23-85)
5-2
5-4
5-8
6-3
6-4
6-7
6-8
7-1
7-2
7-3
8-1
8-2
8-3
8-4
8-5
8-6
9-1 | Internal failure of the SRS unit. If intermittent, could mean internal failure of the unit or a faulty indicator light circuit. Refer to Troubleshooting Intermittent Failures (see page 23-38). | (see page 23-85)
9-2 | Internal failure of the SRS unit. If intermittent, could mean internal failure of the power supply (VB line). Refer to Troubleshooting Intermittent Failures (see page 23-38).
9-6 | Faulty left front sensor | (see page 23-88)
9-7 | Faulty right front sensor | (see page 23-91)
10-1 | Seat belt tensioners (and airbag(s)) deployed | (see page 23-85)