## Fuel and Emissions Systems

#### DTC Troubleshooting Index (cont'd)

11-7

DTC | Indicator Lamp | Detection Item | Page
Scan tool DTC | Honda DTC | MIL (Check Engine Lamp) | Glow Lamp
P1086 | - | On | On | Rail Pressure Control System High Performance | (see page 11-92)
P1087 | - | On | On | Rail Pressure Low | (see page 11-94)
P1088 | - | On | On | Rail Pressure High | (see page 11-96)
P1091 | - | On | On | Rail Pressure Control Valve (Fuel Metering Unit) Circuit Open | (see page 11-98)
P1092 | - | On | On | Rail Pressure Control Valve (Fuel Metering Unit) Circuit Short | (see page 11-99)
P1095 | - | On | On | Rail Pressure Control System Low Performance | (see page 11-100)
P1100 | - | On | - | MAF Sensor Supply Voltage High/Low | (see page 11-102)
P1101 | - | On | - | Incorrect MAF High Range | (see page 11-104)
P1104 | - | On | - | Incorrect MAF Low Range | (see page 11-106)
P1107 | - | On | - | BARO Sensor Circuit Low Voltage | (see page 11-107)
P1108 | - | On | - | BARO Sensor Circuit High Voltage | (see page 11-108)
P1112 |  | On | - | Variable Swirl Control Valve Circuit Open | (see page 11-167)
P1113 | - | On | - | Variable Swirl Control Valve Circuit Short | (see page 11-168)
P1195 | - | On | On | Fuel Pressure Sensor Supply Voltage High/Low | (see page 11-108)
P1224 | - | On | On | Accelerator Pedal Position (APP) Sensor 1 Supply Voltage High/Low | (see page 11-110)
P1229 | - | On | On | Accelerator Pedal Position (APP) Sensor 2 Supply Voltage High/Low | (see page 11-112)
P1235 | - | On | - | MAP Sensor Supply Voltage High/Low | (see page 11-114)
P1236 | - | On | - | Boost Pressure Control Negative Deviation | (see page 11-115)
P1237 | - | On | - | Boost Pressure Control Positive Deviation | (see page 11-116)
P1238 | - | On | - | Boost Pressure Control Circuit Open | (see page 11-117)
P1239 | - | On | - | Boost Pressure Control Circuit Short | (see page 11-118)
P1248 | - | On | On | Accelerator Pedal Position (APP) Sensor 1 and 2 Comparison | (see page 11-119)
P1331 | - | On | On | CKP-CMP Correlation Dynamic Implausible | (see page 11-120)
P1377 | - | On | - | Glow Time Control Circuit Open | (see page 11-122)
P1378 | - | On | - | Glow Time Control Circuit Short | (see page 11-123)
P1401 | - | On | - | EGR Valve Control Negative Deviation | (see page 11-173)
P1403 | - | On | - | EGR Valve Control Circuit Open | (see page 11-175)
P1404 | - | On | - | EGR Valve Control Circuit Short | (see page 11-176)

a a a