## Manual Transmission

#### Mainshaft Reassembly

13-30

Exploded View

1. 3RD/4TH SYNCHRO SLEEVE
2. ANGULAR BALL BEARING

   Check for wear and operation.

   Note the direction of installation.

3. 6TH GEAR
4. NEEDLE BEARING

   Check for wear and operation.

5. DISTANCE COLLAR
6. DOUBLE CONE SYNCHRO
7. SYNCHRO SPRING
8. 5TH/6TH SYNCHRO SLEEVE
9. 5TH/6TH SYNCHRO HUB
10. SYNCHRO SPRING
11. DOUBLE CONE SYNCHRO
12. 5TH GEAR
13. NEEDLE BEARING

    Check for wear and operation.

14. 4TH GEAR
15. DOUBLE CONE SYNCHRO
16. SYNCHRO SPRING
17. DISTANCE COLLAR
18. MAINSHAFT
19. NEEDLE BEARING

    Check for wear operation.

20. 3RD GEAR
21. DOUBLE CONE SYNCHRO
22. SYNCHRO SPRING
23. 3RD/4TH SYNCHRO HUB

a a a