## Seats

#### Front Seat Cover Replacement (cont'd)

20-4

1. Remove the rear seat access knob (A) and screw and release the hook (B), then remove the rear seat access trim (C).

1. Pull back the seat-back cover (A) all the way around and release the clips (B).

1. Using a flat-tip screwdriver wrapped with protective tape, insert a flat-tip screwdriver to the hook portions (seven places) of the headrest rear trim (A) from the headrest front trim side. Pry up the hooks (B) to release the tabs (C) of the headrest front trim (D) while pulling the headrest front trim forward and remove the trim.

a a a