## Power Distribution

#### Fuse to Components Index (cont'd)

22-44

Under - dash Fuse/Relay Box

Fuse Number | Amps | Wire Colour | Component(s) or Circuit(s) Protected
1 | 15A | BLK/WHT | Ignition coils
2 | ——— | ——— | Not used
3 | 10A | Fuse/relay box socket | Multiplex control unit (KG model: daytime running lights)
20A | BLU/RED | Front fog light (KH model), Front fog light indicator light (KH model)
4 | 10A | BLK/ORN | Alternator, Cruise control unit, Cruise main switch, ELD unit (KU model), EVAP purge control solenoid valve, Primary HO2S, Secondary HO2S, Vehicle speed sensor
5 | 7.5A | Fuse/relay box socket | Multiplex control unit (KG model, KB model, KH model, TR model, KE model)
6 | 7.5A | YEL/GRN | Headlight adjuster switch, Headlight adjuster unit, Power window master switch, Sunroof open relay, Sunroof close relay
7 | 20A | GRN | Sunroof motor
8 | 7.5A | Fuse/relay box socket | Optional connector V, Multiplex control unit
YEL/RED | Audio unit, Key interlock relay (KH model), Key interlock solenoid (KH model)
9 | 10A | GRN | OPDS unit
10 | 7.5A | Fuse/relay box socket | Multiplex control unit
YEL | A/T reverse relay, Back-up lights, EPS control unit, Gauge assembly, Keyless receiver unit, Security control unit (KG model: 1.6 ES, KH model, KK model: EX, KX model, TR model: 1.6 ES, KN model), Shift lock relay (KH model), Shift lock solenoid (KM model: A/T, KP model: A/T, KX model: A/T, KQ model: A/T)
11 | 7.5A | BLK/ORN | ABS modulator-control unit
12 | 7.5A | Fuse/relay box socket | Multiplex control unit (KG model: daytime running lights)
13 | 10A | PNK | SRS unit
14 | 10A | Fuse/relay box socket | Optional connector V
BLK/YEL | A/C compressor clutch relay, Blower motor relay, Condenser fan relay, Climate control unit (with auto A/C), Heater control panel (without auto A/C), Power mirror actuator, Power mirror defogger, Radiator fan relay, Rear window defogger relay, Recirculation control motor, Seat heater main relay
15 | 10A | WHT | Security control unit connector (optional)
30A | RED/YEL | Headlight washer control unit
16 | 20A | RED/BLK | Driver's seat heater, Passenger's seat heater
17 | 15A | BLK/YEL | Inertia switch (KG model, KB model, TR model, KE model), SRS unit
YEL/BLK | ECM, PCM, Fuel pump
18 | 15A | YEL/GRN | Cigarette lighter
19 | 7.5A | YEL/BLK | Turn signal/hazard relay
20 | 20A | Fuse/relay box socket | Multiplex control unit
GRN/BLK | Windshield wiper motor, Windshield washer motor
21 | ——— | ——— | Not used
22 | 20A | GRN/BLK | Front passenger's power window motor
23 | 20A | GRN/WHT | Driver's power window motor
24 | 20A | YEL/RED | Left rear power window motor
25 | 20A | YEL/BLU | Right rear power window motor