## Stereo Sound System

#### Speaker Replacement

22-31

Tweeter:

1. Remove the door panel (see page 20-4).
2. Disconnect the 2P connector (A) from the tweeter (B).

3. Remove the mirror garnish (C).
4. Remove the screw and tweeter from the mirror garnish.

Rear Speaker:

1. Remove the rear shelf (see page 20-35).
2. Remove the four screws, and disconnect the 2P connector (A) from the speaker (B).