## Lubricants and Fluids

####

3-2

For the details of lubrication points and type of lubricants to be applied, refer to the illustrated index and various work procedures (such as Assembly/Reassembly, Replacement, Overhaul, Installation, etc.) contained in each section.

NO. | LUBRICATION POINTS | LUBRICANT
1 | Engine | Always use fuel-efficient that says "API service SG, SH or SJ" SAE Viscosity See chart below.
2 | Transmission | Manual | Genuine Honda Manual Transmission Fluid (MTF) *1
Automatic | Genuine Honda ATF-Z1 (ATF) *2
3 | Brake system (includes ABS line) | Brake fluid DOT 3 or DOT 4 *3
4 | Clutch line | Brake fluid DOT 3 or DOT 4 *3
5 | Power steering gearbox | Steering grease P/N 08733-B070E
6 7 | Release fork (manual transmission) Shift and select cable ends (Manual transmission) | Super High Temp Urea Grease (P/N 08798-9002)
8 | Throttle cable end (dashboard lower panel hole) | Silicon grease
9 10 11 12 13

14

15

Throttle cable end (throttle link)

Brake master cylinder pushrod

Clutch master cylinder pushrod

Shift lever

Pedal linkage

Battery terminals

Fuel fill lid

Multi-purpose grease
16 17 18 19 20 | Rear brake shoe linkage Hood hinges and latch Tailgate hinges and latch Door hinges, upper and lower Door opening detent | Honda White Lithium Grease
21 | Calliper piston boot, calliper pins and boots | Silicone grease
22 | Brake line joints (front and rear wheelhouse) | Rust preventatives
23 | Air conditioning compressor | Compressor oil: SANDEN: SP-10 (P/N 38897-P13-003 or 38899-P13-A01) For refrigerant: HFC-134a (R-134a)

CAUTION Used engine oil may cause skin cancer if repeatedly left in contact with the skin for prolonged periods. Although this is unlikely unless you handle used oil on a daily basis, it is still advisable to thoroughly wash your hands with soap and water as soon as possible after handling used oil.

*1: Always use genuine Honda Manual Transmission Fluid (MTF). Using motor oil can cause stiffer shifting because it does not contain the proper additives.

*2: Always use genuine Honda ATF-Z1 (ATF). Using a non-Honda ATF can affect shift quality.

*3: We recommend Genuine Honda Brake Fluid. Using a non-Honda brake fluid can cause corrosion and decrease the life of the system.