## Stereo Sound System

#### Audio Unit Connector Replacement

22-30

Cavity | Wire | Connects to
1 | YEL/GRN | Antenna module
2 | YEL/RED | ACC (Main stereo power supply)
3 | - | Not used
4 | - | Not used
5 | PNK | Right rear speaker (+)
6 | BLU/WHT | Left rear speaker (+)
7 | GRN/YEL | Passenger's door speaker (+), Right tweeter (+)
8 | GRN/BLK | Driver's door speaker (+), Left tweeter (+)
9 | RED/BLK | Lights-on signal
10 | WHT/RED | Constant power
11 | - | Not used
12 | - | Not used
13 | - | Not used
14 | - | Not used
15 | BLU/YEL | Right rear speaker (-)
16 | BLU/BLK | Left rear speaker (-)
17 | GRY/RED | Passenger's door speaker (-), Right tweeter (-)
18 | LT GRN | Driver's door speaker (-), Left tweeter (-)
19 | RED | Dash lights brightness controller
20 | BLK | Ground (G503)

AUDIO UNIT 20P CONNECTOR