# FRONT DOOR > THREE-DIMENSIONAL DISTANCE

HINT:

1. In cases in which only one dimension is given, left and right are symmetrical.

1. For symbols, capital letters indicate right side of vehicle, small letters indicate left side of vehicle (seen from rear).

Measuring Point Name
Symbol | Name | Hole Diameter mm (in.)
A, a | Roof Panel Corner | -
B, b | Hood Hinge Installation Nut | M8 (0.31)
C, c | Front Door Hinge Installation Nut | M8 (0.31)
D, d | Front Door Hinge Installation Nut | M8 (0.31)
E, e | Front Body Pillar Assembly Mark | -
F, f | Front Body Pillar Assembly Mark | -
G, g | Front Body Pillar Assembly Mark | -
H, h | Rocker Panel Assembly Mark | -
J, j | Rocker Panel Assembly Mark | -
K, k | Roof Side Rail Assembly Mark | -
L, l | Center Body Pillar Assembly Mark | -
M, m | Center Body Pillar Assembly Mark | -
N, n | Front Door Lock Striker Installation Nut | M8 (0.31)
O, o | Rear Door Hinge Installation Nut | M8 (0.31)
P, p | Rear Door Hinge Installation Nut | M8 (0.31)
Q, q | Rocker Panel Assembly Mark | -