# ENGINE COMPARTMENT REFERENCE VALUES > THREE-DIMENSIONAL DISTANCE

HINT:

1. Measure points with the radiator support opening cover and front fender reinforcement top removed.
2. In cases in which only one dimension is given, left and right are symmetrical.

1. For symbols, capital letters indicate right side of vehicle, small letters indicate left side of vehicle (seen from rear).

Measuring Point Name
Symbol | Name | Hole Diameter mm (in.)
A, a | Radiator Grille Installation Bolt | M6 (0.24)
B, b | Headlight Installation Screw | -
C, c | Headlight Installation Screw | -
D, d | Front Fender Installation Bolt | M6 (0.24)
E, e | Front Fender Installation Bolt | M6 (0.24)