#
AUDIO SYSTEM OUTLINE

BME092000001T01
• The vehicle is equipped with an audio unit, speakers glass antennas, and an antenna feeder.
• The audio unit consists of the following parts:

  - Base unit, which has AM/FM tuner and control function for each module
  - Upper module (CD player or CD changer)
  - Lower module (cassette deck or MD player)
  - Cover

• The upper module (CD player or CD changer) and lower module (cassette deck or MD player) are options.
• Module availability depends on vehicle grade.
• The operation of audio unit is the same as that of current XEDOS 9, MILLENIA (TA) models.
• The audio control switch has been added to the steering wheel. (Button type or lever type)

## Speaker System

• In the new 8-speaker system, the tweeters, which are placed at both the front and rear of the room, provide a clear, high frequency sound.
• A soft dome front tweeter with a PPS (Polyphenylene Sulfide) diaphragm had been adopted for a wide band width and clear high frequency sound without distortion.