#
DTC 03 ERR07 OR 03:ER07

BME090266900W14

DTC 03 ERR07 or 03:Er07 | CD player
DETECTION CONDITION |

  Note

  • When error occurs, error message "CHECK CD" is displayed in the LCD.

• Base unit detects CD reading error.
POSSIBLE CAUSE | • Defective CD (scratches or dirt) • CD player malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | INSPECT CD • Inspect condition of CD where error has occurred. • Is CD okay? | Yes | Go to next step.
No | Repair (remove foreign material) or replace CD, then go to next step.
2 | INSPECT CD PLAYER • Clear DTC. • Insert and play CD with no defect. • Start on-board diagnostic test mode. • Is DTC 03 ERR07 or 03:Er07 displayed? | Yes | Replace CD player.
No | Troubleshooting completed.