#
FORWARD CLUTCH, 3-4 CLUTCH HYDRAULIC CIRCUIT OUTLINE

BME051719500104

• By designing exclusive passages for the forward clutch and the 3-4 clutch in the transaxle case, via the oil pump and end cover, the hydraulic pressure passages are shortened and control during clutch engagement is improved.

.

1 | Oil pump
2 | Forward clutch hydraulic passage
3 | Forward clutch
4 | End cover
5 | 3-4 clutch hydraulic passage
6 | 3-4 clutch