#
NO.25 ENGINE STALLS WHEN DRIVING AT SLOW SPEEDS OR STOPPING [FN4A-EL]

BME050301030229

25 | Engine stalls when driving at slow speeds or stopping
DESCRIPTION | • Engine stalls when brake pedal is depressed while driving at low speed or stopping.
POSSIBLE CAUSE | • The malfunction is in engine control system (e.g. Fuel injection control, IAC system). Otherwise, the malfunction is in the control valve body, shift solenoid E or TCC.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | Go to No.10 "LOW IDLE/STALLS DURING DECELERATION". (See NO.10 LOW IDLE/STALLS DURING DECELERATION [L3].) Is the engine control system normal? | Yes | Go to the next step.
No | Repair or replace any malfunctioning parts according to the inspection results.
2 | Go to No.5 "ENGINE STALLS-AFTER START/AT IDLE". (See NO.5 ENGINE STALLS-AFTER START/AT IDLE [L3].) Is the engine control system normal? | Yes | Repeat the basic inspection and repair or replace any malfunctioning parts according to the inspection result. (See BASIC INSPECTION [FN4A-EL].)
No | Repair or replace any malfunctioning parts according to the inspection results.