#
FRONT DRAIN HOSE INSTALLATION

BME091569920W02

  Caution

  • If the front drain hose is pinched or bent anywhere, the water in the hose may not discharge and enter the inside of the vehicle. During and after installation of the trims and the headliner, always make sure there is no interference with the front drain hose. Fix any problem if found.

1. Apply soapy water to the front drain hose inserting area.

2. Insert one end (the wider end) of the front drain hose into the sunroof frame.

3. Install the front drain hose to the clips, parallel to the pillar and free of slack.

4. Insert the front drain hose joint into the hinge pillar inner hole.

5. Install the headliner.