#
ENGINE CONTROL SYSTEM WIRING DIAGRAM [MZR-CD (RF Turbo)]

BME014000140T19

.

1 | PCM
2 | DLC
3 | DLC-2
4 | Water heater unit
5 | Fuel pump
6 | IDM
7 | Battery
8 | Engine switch
9 | Starter
10 | Generator
11 | Generator warning light
12 | Neutral switch
13 | Clutch switch
14 | Oil pressure switch
15 | VSS
16 | Glow indicator light
17 | MIL
18 | Instrument cluster
19 | Sedimentor switch
20 | Immobilizer unit
21 | PCM control relay
22 | MAF/IAT sensor

.

23 | Fuel injector No.1
24 | Fuel injector No.2
25 | Fuel injector No.3
26 | Fuel injector No.4
27 | Calibration resistor No.1
28 | Calibration resistor No.2
29 | Calibration resistor No.3
30 | Calibration resistor No.4
31 | CMP sensor
32 | CKP sensor
33 | EGR control solenoid valve
34 | EGR solenoid valve (vacuum)
35 | EGR solenoid valve (vent)
36 | VSC solenoid valve
37 | Intake shutter solenoid valve (half)
38 | Intake shutter solenoid valve (full)
39 | VBC solenoid valve
40 | Boost sensor
41 | Accelerator position sensor
42 | Idle switch
43 | Fuel pressure sensor
44 | ECT sensor
45 | Fuel temperature sensor
46 | Suction control valve
47 | IAT sensor No.2
48 | Glow plug relay
49 | Glow plug
50 | With fuel warmer
51 | Fuel warmer
52 | Vacuum switch
53 | Main fan relay
54 | Fan control module
55 | Main fan
56 | Additional fan
57 | Refrigerant pressure switch (middle)
58 | Refrigerant pressure switch (low)
59 | A/C switch
60 | A/C amplifier
61 | A/C relay
62 | Refrigerant pressure switch (high)
63 | Magnetic clutch