#
FOREWORD [MZR-CD (RF Turbo)]

BME010200102227
• When the customer reports a vehicle malfunction, check the malfunction indicator light (MIL) indication and diagnostic trouble code (DTC), then diagnose the malfunction according to following flowchart.

  - If the DTC exists, diagnose the applicable DTC inspection. (See DTC TABLE [MZR-CD (RF Turbo)].)
  - If the DTC does not exist and the MIL does not illuminate or flash, diagnose the applicable symptom troubleshooting.
  *: Malfunction Indicator Light (MIL), Generator Warning Light, Security Light