#
INPUT/TURBINE SPEED SENSOR DESCRIPTION [JA5A-EL]

BME051719200T08

## Function

• A input/turbine speed sensor is located in the transaxle case and detects the rotating speed of the reverse clutch drum.

## Construction/Operation

• The magnetic pickup type of input/turbine speed sensor is mounted in the transaxle case, next to the reverse clutch drum. It generates a 36-pulse signal for each rotation of the reverse clutch drum, and sends this signal to the TCM.