#
REAR AIRFLOW MODE AND AIR MIX ACTUATOR CONSTRUCTION

BME074061072T01

## Vehicle With Rear Climate Control Unit (Two Dial Type)

• A mode and air mix actuator, integrating a mode actuator and air mix actuator, has been adopted.
• Based on the signal from the rear heater control unit, the mode door and air mix door are moved so that the airflow corresponds to either cold air in vent mode or hot air in heat mode.