#
ENGINE CONTROL SYSTEM DIAGRAM [MZR-CD (RF Turbo)]

BME014000140T18

.

1 | Air cleaner
2 | Vacuum chamber
3 | VBC Check valve
4 | MAF/IAT sensor
5 | VBC solenoid valve
6 | Vacuum damper
7 | Guide blade actuator
8 | Turbocharger
9 | Charge air cooler
10 | IAT sensor No.2
11 | Boost sensor
12 | Intake shutter valve actuator
13 | Intake shutter solenoid valve (half)
14 | Intake shutter solenoid valve (full)
15 | EGR solenoid valve (vacuum)
16 | EGR solenoid valve (vent)
17 | EGR control solenoid valve
18 | EGR valve
19 | EGR water cooler
20 | VSC valve actuator
21 | Fuel tank
22 | Fuel filter
23 | Fuel warmer
24 | Supply pump
25 | Suction control valve
26 | Fuel temperature sensor
27 | Common rail
28 | Fuel pressure sensor
29 | Fuel pressure limiter
30 | Glow plug
31 | Fuel injector
32 | ECT sensor
33 | Calibration resistor
34 | CMP sensor
35 | Warm up oxidation catalytic converter
36 | Oxidation catalytic converter
37 | Silencer
38 | Vacuum pump
39 | CKP sensor
40 | Idle switch
41 | Accelerator position sensor
42 | Glow plug relay
43 | IDM
44 | PCM
45 | BARO sensor
46 | PCM control relay
47 | Engine switch
48 | Starter (starter signal)
49 | Neutral switch
50 | Clutch switch
51 | A/C switch
52 | DLC (TEN)
53 | VSS
54 | CAN Bus
55 | VSC solenoid valve
56 | To PCM