#
EMISSION SYSTEM OUTLINE [AJ]

BME011600000T06
• The emission system for Mazda MPV has been adopted or changed the following parts.

  - Due to the layout change in the exhaust system, a TWC has been added.

Item | Remark for new model
--- | ---
Purge solenoid valve | Same function as previous MPV (LW) GY engine models
Catch tank | Same as previous MPV (LW) GY engine models
Evaporative check valve | Same as previous MPV (LW) GY engine models
Charcoal canister | Same as previous MPV (LW) GY engine models
Rollover valve | Same as previous MPV (LW) GY engine models
EGR valve | Same as previous MPV (LW) GY engine models
WU-TWC | Same function as previous MPV (LW) GY engine models
TWC | Same function as WU-TWC of previous MPV (LW) GY engine models
Oil separator | Same as previous MPV (LW) GY engine models
PCV valve | Same as previous MPV (LW) GY engine models
Ventilation hose | Same function as previous MPV (LW) GY engine models