#
SLOPE MODE CONTROL OPERATION [FN4A-EL]

BME051718880T28

## Climbing hill

• When the hill is steeper than a specified grade, unnecessary shift up is prevented by holding an appropriate shift gear.

## Descending hill

• When the descent is steeper than a specified grade and the brake switch is depressed, use of the brake pedal is reduced by shifting from 4GR to 2GR and applying the engine brake effectively.