#
DTC 05 ERR01 OR 05:ER01

BME090266900218

DTC 05 ERR01 or 05:Er01 | CD changer (external type)
DETECTION CONDITION | • Changer function does not operate.
POSSIBLE CAUSE | • Defective CD (broken or foreign material) • Magazine malfunction • CD changer (external type) malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY WHETHER MALFUNCTION IS IN CD CHANGER OR OTHER PARTS • Operate changer function. • Is function okay? | Yes | Go to Step 4.
No | Not able to change particular CD. | Go to next step.
Not able to change any CD. | Go to Step 3.
2 | INSPECT CD • Inspect condition of CD where error has occurred. • Is CD okay? | Yes | Go to next step.
No | Repair (remove foreign material) or replace CD, then go to next step.
3 | INSPECT MAGAZINE • Inspect magazine. • Is magazine okay? | Yes | Go to next step.
No | Repair or replace magazine, then go to next step.
4 | INSPECT CD CHANGER (EXTERNAL TYPE) • Clear DTC. • Operate changer. • Start on-board diagnostic test mode. • Is DTC 05 ERR01 or 05:Er01 displayed? | Yes | Replace CD changer (external type).
No | Troubleshooting completed.