#
OPEN LOCK STRUCTURAL VIEW

BME091101085T08
• When the sliding door is opened fully, the door is held at the fully open position so that it does not slide in the close direction.
• As the cable is linked with the outer and inner handles, the cable is pulled when either handle is operated (1). Due to this, the latch is released, and the sliding door moves.

.

1 | Lower roller
2 | Open lock
3 | Striker
4 | Body
5 | Close slide
6 | Cable
7 | Latch