#
CONTROL VALVE BODY OUTLINE

BME051721100101

• The control valve body is composed of three bodies: the upper control valve body, main control valve body, and the solenoid control valve body.

• Because the clutch engagement pressure is controlled electronically, the hydraulic circuits are simplified, the valve types are reduced, and the control valve body is miniaturized.

• The nonwoven fabric oil strainer is installed in the control valve body to prevent contamination.

1 | Upper control valve body
2 | Main control valve body
3 | Oil strainer
4 | Solenoid valve body
5 | Shift solenoid A
6 | Shift solenoid B
7 | Shift solenoid C
8 | Shift solenoid D
9 | Shift solenoid E
10 | Pressure control solenoid