#
INPUT/OUTPUT SIGNAL AND RELATED CONTROLS [FN4A-EL]

BME051718880T06

Component | Control item
--- | ---
Line pressure control | Shift control | Clutch pressure direct control (Direct electric shift control) | Feedback control | Engine-transaxle total control | Torque converter clutch control | Slope mode control | On-board diagnostic function
Input
HOLD switch |  | X |  |  |  |  |  |
TR switch | X | X | X |  |  |  |  |
TP sensor | X | X | X |  |  | X |  | X
Input/turbine speed sensor | X | O | X | X |  | X |  | X
Oil pressure switch |  | X | X |  |  |  |  |
VSS | X | X | X |  |  | X | X | X
Brake switch |  |  |  |  |  |  | X |
TFT sensor | X | X | X | X |  | X |  | X
ECT sensor |  |  |  |  |  | X |  | X
CKP sensor | X |  | X |  | X | X |  | X
MAF sensor | X |  | X | X | X |  | X | X
Output
Pressure control solenoid | X |  |  |  |  |  |  | X
Shift solenoid A |  | X | X | X |  | X | X | X
Shift solenoid B |  | X | X | X |  |  |  | X
Shift solenoid C |  | X | X | X |  |  |  | X
Shift solenoid D |  | X |  |  |  |  | X | X
Shift solenoid E |  | X |  |  |  | X | X | X
HOLD indicator light |  | X |  |  |  |  |  | X
Speedometer signal |  |  |  |  |  |  |  |

  X :
Available
  O :
Back up