#
TRANSFER CLEANING

BME051527500M01

## Cleaning Precautions

1. Clean the surface of the transfer using steam and cleaning fluids when disassembly.

  Warning

  • Always wear safety glasses when using compressed air since the foreign material could be blown by the compression air and damage your eyes.

2. Clean removed components with cleaning fluids and use compressed air to blow off the oil. Clean the oil holes and passages with compressed air.