#
CONTROL SYSTEM WIRING DIAGRAM [AJ] (VIN: JMZ LW19J7*# 300001-, JM0 LW10J300 300001-301405, JM6 LW10J300 300001-, JM8 LW28J**# 300001-301513)

BME014000000T55

## With Immobilizer System

## Without Immobilizer System

1 | Battery
2 | Main fuse
3 | Starter
4 | Generator
5 | Ignition switch
6 | DLC
7 | To ABS/TCS HU/CU
8 | Instrument cluster
9 | Main relay
10 | Fuel pump relay
11 | Fuel pump unit
12 | PSP switch
13 | HO2S (front, RH) (integrated with rear HO2S heater)
14 | HO2S (front, LH) (integrated with front HO2S heater)
15 | HO2S (rear, RH) (integrated with rear HO2S heater) (European (L.H.D.) specs.)
16 | HO2S (rear, LH) (integrated with front HO2S heater) (European (L.H.D.) specs.)
17 | EGR valve
18 | MAF/IAT sensor
19 | DLC-2
20 | Generator warning light
21 | MIL
22 | Blower motor
23 | PCM
24 | A/C relay
25 | A/C switch
26 | A/C amplifier
27 | Refrigerant pressure switch (low and high pressure)
28 | Refrigerant pressure switch (middle pressure)
29 | A/C compressor
30 | Fan relay
31 | Fan motor
32 | Fan control module
33 | Fan switch
34 | Microcomputer (DIS)
35 | Immobilizer unit
36 | IAC valve
37 | Purge solenoid valve
38 | ECT sensor
39 | TP sensor
40 | BARO sensor (European (L.H.D.) specs.), EGR boost sensor (Australian, General (L.H.D. R.H.D.) specs.)
41 | EGR boost sensor solenoid valve (used for Australian, General (L.H.D. R.H.D.) specs.)
42 | Intake manifold communication control (IMCC) actuator
43 | CMP sensor
44 | CKP sensor
45 | Fuel injector No.1
46 | Fuel injector No.2
47 | Fuel injector No.3
48 | Fuel injector No.4
49 | Fuel injector No.5
50 | Fuel injector No.6
51 | Condenser
52 | Ignition coil No.1
53 | Ignition coil No.2
54 | Ignition coil No.3
55 | Ignition coil No.4
56 | Ignition coil No.5
57 | Ignition coil No.6
58 | Brake light
59 | Brake switch
60 | To TR switch
61 | Knock sensor
62 | To battery
63 | To instrument cluster
64 | With A/C
65 | Without A/C
66 | European (L.H.D.) specs.
67 | Australian, General (L.H.D. R.H.D.) specs.
68 | Australian specs.
69 | To IG1
70 | To TCM
71 | To main relay terminal A
72 | To PCM terminal 17
73 | To PCM terminal 41
74 | To PCM terminal 69
75 | To PCM terminal 8
76 | To PCM terminal 44
77 | To PCM terminal 56
78 | To PCM terminal 46
79 | To PCM terminal 72
80 | To PCM terminal 12
81 | To EGR valve
82 | To A/C system
83 | To fan control module