#
TRANSMISSION/TRANSAXLE ABBREVIATIONS

BME050001024T01

ATF | Automatic Transaxle Fluid
ATX | Automatic Transaxle
B+ | Battery Positive Voltage
CCM | Comprehensive Component Monitor
CPU | Central Processing Unit
DC | Drive Cycle
DLC | Data Link Connector
DTC | Diagnostic Trouble Code
EC-AT | Electronically Controlled Automatic Transaxle
GND | Ground
MIL | Malfunction Indicator Lamp
MTX | Manual Transaxle
O/D | Overdrive
OBD | On-board Diagnostic
PCM | Powertrain Control Module
PID | Parameter Identification
TCC | Torque Converter Clutch
TFT | Transaxle Fluid Temperature
TP | Throttle Position
TR | Transaxle Range
VSS | Vehicle Speed Sensor
1GR | First Gear
2GR | Second Gear
3GR | Third Gear
4GR | Fourth Gear