#
CONNECTING ROD, CONNECTING ROD BEARING [MZR-CD (RF Turbo)]

BME011011211T02

## Structure

• Connecting rods are made of carbon steel.
• Dowel pins are used to position the rod cap to the connecting rod.
• Connecting rod caps are secured with plastic region bolts.

1 | Bush
2 | Connecting rod upper bearing
3 | Connecting rod lower bearing
4 | Connecting rod cap
5 | Connecting rod
6 | Dowel pin
7 | Connecting rod cap bolt (plastic region bolts)
8 | Alignment marks