#
CHILD SEAT ANCHOR INSTALLATION

BME081157620203

## Australian Specs. Only

  Note

  • The child seat anchor is available as a service part. Perform the following procedure to install the child seat anchor behind the third-row left seat.

1. Cut the carpet going around the hole in the trunk board.

2. Cut out the trunk board.

3. Peel back the rear floor covering.

4. Remove the seal.

5. Install the child seat anchor.