#
CALIBRATION RESISTOR CONSTRUCTION [MZR-CD (RF Turbo)]

BME014013251T02
• The resistor is built into each calibration resistor of the fuel injectors.
• There are 25 types of calibration resistors according to fuel injection amount deviations.
• Fuel injectors and calibration resistors of the same rank are to be matched respectively as shown in the table below.

Reference table

Fuel injector rank number | Calibration resistor
--- | ---
Rank number | Resistance (ohm)
1 | 1 | 30.9
2 | 2 | 41.2
3 | 3 | 53.6
4 | 4 | 68.1
5 | 5 | 84.5
6 | 6 | 105
7 | 7 | 130
8 | 8 | 158
9 | 9 | 196
10 | 10 | 243
11 | 11 | 301
12 | 12 | 365
13 | 13 | 442
14 | 14 | 549
15 | 15 | 665
16 | 16 | 825
17 | 17 | 1020
18 | 18 | 1240
19 | 19 | 1540
20 | 20 | 1920
21 | 21 | 2370
22 | 22 | 3010
23 | 23 | 4020
24 | 24 | 5760
25 | 25 | 9530

.

1 | Calibration resistor
2 | Resistor
3 | Fuel injector
4 | IDM
5 | PCM
6 | Rank number