#
FRONT ABS WHEEL-SPEED SENSOR REMOVAL/INSTALLATION

BME041343720201

1. For left side, remove the air cleaner and air filter. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [L3].) (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [AJ].) (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

1 | Connector
2 | Bolt
3 | Front ABS wheel-speed sensor