#
FUEL SYSTEM LOCATION INDEX [AJ]

BME011400114210

Engine Room Side

Fuel Tank Side

1 | Fuel tank (See FUEL TANK REMOVAL/INSTALLATION [AJ]) (See FUEL TANK INSPECTION [AJ])
2 | Rollover valve (See FUEL TANK INSPECTION [AJ])
3 | Nonreturn valve (See NONRETURN VALVE INSPECTION [AJ])
4 | Fuel pump unit (See FUEL PUMP UNIT REMOVAL/INSTALLATION [AJ]) (See FUEL PUMP UNIT DISASSEMBLY/ASSEMBLY [AJ]) (See FUEL PUMP UNIT INSPECTION [AJ])
5 | Fuel filter (high-pressure) (See FUEL FILTER (HIGH-PRESSURE) REMOVAL/INSTALLATION [AJ])
6 | Pressure regulator (See PRESSURE REGULATOR INSPECTION [AJ])
7 | Fuel injector (See FUEL INJECTOR REMOVAL/INSTALLATION [AJ]) (See FUEL INJECTOR INSPECTION [AJ] (VIN: JMZ LW19J7*# 300001-, JM0 LW10J300 300001-301405, JM6 LW10J300 300001-, JM8 LW28J**# 300001-301513)) (See FUEL INJECTOR INSPECTION [AJ] (VIN: JM0 LW10J300 301406-, JMZ LW69J7*# 307683-, JM8 LW28J**# 301514-, JM8 LW28A**# 301514- (Assumed)))
8 | Fuel-filler cap
9 | Pulsation damper (See PULSATION DAMPER REMOVAL/INSTALLATION [AJ]) (See PULSATION DAMPER INSPECTION [AJ])
10 | Fuel pump relay (See RELAY INSPECTION)
11 | Quick release connector (fuel distributor side)
12 | Quick release connector (engine room side)